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Rl English

a RI-1is a miniature «NO-1»
electromechanical relay with two fuill «COM-1»
groups of contacts. It is designed for NC-1»
concealed installation in the original cai Ground:
wires. It allows to implement blocking
of engine control circuits including «+12V»
shunt method. The relay can be used to «NC-2»
block CAN-bus (it is used to implernent «COM-2»
remote engine start via CAN-bus for NO-2» —m
some cars).

Current consumption — 10mA.
Voltage - 12V.

Enclosure class: P54
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